Le fotometrie fornite fanno riferimento al singolo modulo C-Box M o C-Box L (codici 2631 e 2641).
Per il corretto utilizzo dei file fotometrici al fine di rappresentare modelli contenenti più moduli, creare delle serie lineari come segue:

- C-Box M2 (codice 2632): 2pz in serie lineare lunga 277mm con interdistanza fra il centro dei proiettori di 130mm
- C-Box L2 (codice 2642): 2pz in serie lineare lunga 343mm con interdistanza fra il centro dei proiettori di 170mm
- C-Box M3 (codice 2633): 3pz in serie lineare lunga 414mm con interdistanza fra il centro dei proiettori di 133mm
- C-Box L3 (codice 2643): 3pz in serie lineare lunga 513mm con interdistanza fra il centro dei proiettori di 170mm

The photometric files provided refer to the single C-Box M or C-Box L module (codes 2631 and 2641).
For the correct use of photometric files in order to represent models containing multiple modules, create a linear array as follows:

- C-Box M2 (code 2632): 2pcs in linear array 277mm long with distance between the center of the projectors of 130mm
- C-Box L2 (code 2642): 2pcs in linear array 343mm long with distance between the center of the projectors of 170mm
- C-Box M3 (code 2633): 3pcs in linear array 414mm long with distance between the center of the projectors of 133mm
- C-Box L3 (code 2643): 3pcs in linear array 513mm long with distance between the center of the projectors of 170mm